# 

# **REPUBLIC OF KENYA**

**MINISTRY OF ROADS AND TRANSPORT**

**STATE DEPARTMENT OF ROADS**

Telegraphic Address: “MINWORKS”, Nairobi Materials Testing & Research Division Telephone: Nairobi 0202554950 Machakos Road, Industrial Area Fax: 554877 P.O. Box 11873 – 00400 E-mail: chiefengineer@mtrd.go.ke NAIROBI

Ref No. M.2156/35/L/10 Date: 14th April, 2023

|  |  |
| --- | --- |
| **Laboratory Test Report** |  |

1. **Customer’s Address**: STECOL COPORATION

**E-mail**: martinwanjohi474@gmail.com

1. **Address**: Not provided **Phone**: 0721621952
2. **Customer Contact**: 0721621952 6. **Job Card** **No**.1986/S/2023
3. **Sample Description**: GCS 7. **Date fee paid**: 09/03/2023
4. **Sample by**: Client. 8**. GOK MR No**. 4127763
5. **Date of Sample received**: 09/03/2023 9**. Date Analysis started**:09/03/2023

10. **Additional information provided by the customer**: Kenyatta Road.

**Source:** Kilimanbogo Quarry

|  |
| --- |
|  |
| |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | **S/NO** | **Description** | **Dosage** | **MDD by VH Method** | **OMC** | **PI on Fines** | **Particle Size Distribution,**  **% Passing BS Sieves size (mm)** | | | | | | | | | | | **50** | **37.5** | **28** | **20** | **10** | **6.3** | **2** | **1** | **0.425** | **0.075** | | **(%)** | **Kg/m3** | **(%)** | **(%)** | | 780/S/22 | GCS 0/30 | Neat | 2110 | 6.3 |  | 100 | 100 | 95 | 80 | 55 | 43 | 30 | 24 | 17 | 7 | | **IMPROVED WITH BAMBURI CEMENT 42.5N CEMI 7 DAYS CURE & 7 DAYS SOAK** | | | | | | | | | | | | | | | 1.5% | **LOAD**  **KNs** | **UCS**  **KN/M2** |  |  |  |  |  |  |  |  |  |  |  | | 138.9 | 7653 |  |  |  |  |  |  |  |  |  |  |  | | 165.4 | 9113 |  |  |  |  |  |  |  |  |  |  |  | | 150.8 | 8309 |  |  |  |  |  |  |  |  |  |  |  | | **AV** | **8358** |  |  |  |  |  |  |  |  |  |  |  |     **Eng. J.M. Mbarua**  **For. CHIEF ENGINEER (MATERIALS)**  **OiC Soils Laboratory. CSE Soils Laboratory**  **…………………. ………………** |