# 

# **REPUBLIC OF KENYA**

**MINISTRY OF ROADS AND TRANSPORT**

**STATE DEPARTMENT OF ROADS**

Telegraphic Address: “MINWORKS”, Nairobi Materials Testing & Research Division Telephone: Nairobi 0202554950 Machakos Road, Industrial Area Fax: 554877 P.O. Box 11873 – 00400 E-mail: chiefengineer@mtrd.go.ke NAIROBI

Ref No. M.2360/35/L/10 Date: 17th MAY, 2023

|  |  |
| --- | --- |
| **Laboratory Test Report** |  |

1. **Customer’s Address**: TRANSLEE KENYA LIMITED

**E-mail**: mbindyokawinzi@gmail.com

1. **Address**: P.O BOX 16395-20100 **Phone**:0722455721
2. **Customer Contact**: 0722455721 6. **Job Card** **No**.2368/S/2023
3. **Sample Description**: GCS 0/30 7. **Date fee paid**: 26/04/2023
4. **Sample by**: Client. 8**. GOK MR No**. 4052823
5. **Date of Sample received**: 26/04/2023 9**. Date Analysis started**:27/04/2023

10. **Additional information provided by the customer**: Periodic Maintenance of Kiambu -Riani-Ndenderu (B115) Rd

**Source: Mugoya.**

|  |
| --- |
|  |
| |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | S/NO | Description | Dosage | MDD by VH Method | OMC | PI on Fines | Particle Size Distribution,  % Passing BS Sieves size (mm) | | | | | | | | | | | 50 | 37.5 | 28 | 20 | 10 | 6.3 | 2 | 1 | 0.425 | 0.075 | | (%) | Kg/m3 | (%) | (%) | | 924/S/23 | GCS 0/30 | Neat | 1988 | 6.8 | Non-Plastic | 100 | 100 | 95 | 83 | 65 | 45 | 28 | 16 | 12 | 5 | | IMPROVED WITH MOMBASA CEMENT 42.5N 7 DAYS CURE & 7 DAYS SOAK | | | | | | | | | | | | | | | 2.0% | LOAD  KNs | UCS  KN/M2 |  |  |  |  |  |  |  |  |  |  |  | | 82.0 | 4432 |  |  |  |  |  |  |  |  |  |  |  | | 85.1 | 4518 |  |  |  |  |  |  |  |  |  |  |  | | AV | 4475 |  |  |  |  |  |  |  |  |  |  |  | | 2.5% | 131.3 | 7097 |  |  |  |  |  |  |  |  |  |  |  | | 134.2 | 7394 |  |  |  |  |  |  |  |  |  |  |  | | AV | 7246 |  |  |  |  |  |  |  |  |  |  |  |     Eng. J.M. Mbarua  For. CHIEF ENGINEER (MATERIALS)  OiC Soils Laboratory. CSE Soils Laboratory  …………………. ……………… |