# 

# 

# **REPUBLIC OF KENYA**

**MINISTRY OF ROADS AND TRANSPORT**

**STATE DEPARTMENT OF ROADS**

Telegraphic Address: “MINWORKS”, Nairobi Materials Testing & Research Division Telephone: Nairobi 554950/3/4 Machakos Road, Industrial Area Fax: 554877 P.O. Box 11873 – 00400 E-mail: chiefengineer@mtrd.go.ke NAIROBI

Ref No. M.674/35/L/10 Date:4th October, 2023

|  |
| --- |
|  |

**1. Customer’s Details:** RESIDENT ENGINEER KURA.

**E-mail:** estherwa63@gmail.com

**Address:** P.O. Box 17956-00500 NRB **Phone:** 0721515815

**2. Customer Contact:** 0721515815 6. **Job Card No.** 792/S/2023

**3. Sample Description:** Gravel 7. **Date fee paid:** 26/09/2023

**4. Sampled by:** Client. 8. **GOK MR No**. 4058997

**5. Date Sample received:** 26/09/2023 9. **Date Analysis started**: 29/09/2023

**10. Additional information provided by the customer:** Rehabilitation of Kenyatta national hospital Roads.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | TEST RESULTS | | | | | | | | | | | | | | | | |
| **Sample No.** | **Reference** | **Dosage**% | **Grading** | | | | | | **Atterberg Limits** | | | | | **Compaction T180** | | **CBR** | |
| % Passing BS Sieve Size (mm) | | | | | | LL | PL | PI | LS | PM |  | OMC (%) | 4days Soak  (%) | Swell (%) |
| 20 | 10 | 5 | 2 | 0.425 | 0.075 | % | % | % | % |  | MDD  Kg/m3 |
| 379/S/23 | Gravel for Walkway | Neat | 100 | 98 | 88 | 72 | 58 | 45 | 40 | 27 | 14 | 7 | 812 | 1780 | 16.6 | 25 | 0.3 |
| **SOIL COMPOSITION: Gravel = 28%, Sand = 27%, Silt/clay =45%** | | | | | | | | | | | | | | |

**Eng. J. M. Mbarua**

**For: CHIEF ENGINEER (MATERIALS)**

**OiC Soils Laboratory CSE Soils Laboratory**

**………………. …………………….**