# 

# 

# **REPUBLIC OF KENYA**

**MINISTRY OF ROADS AND TRANSPORT**

**STATE DEPARTMENT OF ROADS**

Telegraphic Address: “MINWORKS”, Nairobi Materials Testing & Research Division Telephone: Nairobi 554950/3/4 Machakos Road, Industrial Area Fax: 554877 P.O. Box 11873 – 00400 E-mail: chiefengineer@mtrd.go.ke NAIROBI

Ref No. M.348/35/L/10 Date: 17th August, 2023

|  |
| --- |
|  |

**1. Customer’s Details:** RESIDENT ENGINEER KeNHA.

**E-mail:** rd.nairobi@kenha.co.ke

**Address:** P.O. Box 200-00507 NRB **Phone:** 0713141871

**2. Customer Contact:** 0713141871 6. **Job Card No.** 216/S/2023

**3. Sample Description:** Wearing Course Layer 7. **Date fee paid:** 27/07/2023

**4. Sampled by:** MTRD Staff. 8. **GOK MR No**. 4053982

**5. Date Sample received:** 10/08/2023 9. **Date Analysis started**:10/08/2023

**10. Additional information provided by the customer: Routine Maintenance and spot Improvement of Isinya-Konza (JNA8) (B50) Road.**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Sample No.** | **Date tested** | **Chainage**  **(Km)** | **Position** | **Layer Thickness (mm)** | **Field dry density**  **Kg/m3** | **Field moisture content (%)** | **Max. dry density**  **T180**  **Kg/m3** | **Optimum moisture content (%)** | **Relative Compaction (%)** | **Relative moisture content (%)** |
| **Base layer Km 0+670-2+100 Wearing Course Layer** | | | | | | | | | | |
| 104/S/23 | 10/08/23 | 0+700 | LHS | 150 | 1626 | 10.5 | 1844 | 12.4 | 88 | 85 |
| 105/S/23 | 10/08/23 | 0+850 | CL | 145 | 1496 | 9.6 | 1844 | 12.4 | 81 | 77 |
| 106/S/23 | 10/08/23 | 1+000 | RHS | 140 | 1397 | 9.3 | 1844 | 12.4 | 76 | 75 |
| 107/S/23 | 10/08/23 | 1+150 | CL | 145 | 1624 | 9.7 | 1844 | 12.4 | 88 | 78 |
| 108/S/23 | 10/08/23 | 1+300 | LHS | 150 | 1480 | 9.2 | 1844 | 12.4 | 80 | 74 |

**Eng. J. M. Mbarua**

**For: CHIEF ENGINEER (MATERIALS OiC Soils Laboratory. CSE Soils Laboratory.**

**………………………. ………………………..**