

**REPUBLIC OF KENYA**

**MINISTRY OF ROADS AND TRANSPORT**

**STATE DEPARTMENT OF ROADS**

Telegraphic Address: “MINWORKS”, Nairobi Materials Testing & Research Division Telephone: Nairobi 0202554950 Machakos Road, Industrial Area Fax: 554877 P.O. Box 11873 – 00400 E-mail: [chiefengineer@mtrd.go.ke](mailto:chiefengineer@mtrd.go.ke) **NAIROBI**

Ref No. M.1886/35/L/10 Date: 8th March, 2023

|  |
| --- |
| **Laboratory Test Report** |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **1. Customer’s Details:** KENYA AIRPORTS AUTHORITY /HAMETHYST LIMITED  **E-mail:** Not provided  **Address:** P.O.BOX 57653-00200 NAIROBI Phone: 0725337459  **2. Customer Contact:** 0725337459 6. Job Card No. 1926/S/2023  **3. Sample Description:** Subbase 2 Layer 7. Date fee paid: 03/03/2023  **4. Sampled by:** MTRD Staff. 8. GOK MR No.4127713  **5. Date Sample received:** 03/03/2023 9. Date Analysis started:03/03/2023  **10. Additional information provided by the customer:** Proposed Musa Gate Access Road and Civil Works JKIA.  **Contract No.** KAA/ES//JKIA/0199/C     |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | **Sample No.** | **Date tested** | **Chainage**  **(Km)** | **Position** | **Layer Thickness (mm)** | **Field dry density**  **Kg/m3** | **Field moisture content (%)** | **Max. dry density**  **T180**  **Kg/m3** | **Optimum moisture content (%)** | **Relative Compaction (%)** | **Relative moisture content (%)** | | **Subbase 2-layer Km0+000-0+140 FW** | | | | | | | | | | | | 774/S/22 | 03/3/2023 | 0+020 | LHS | 150 | 1735 | 14.4 | 1786 | 14.6 | 101 | 99 | | 775/S/22 | 03/3/2023 | 0+060 | CL | 145 | 1783 | 14.3 | 1786 | 14.6 | 99 | 98 | | 776/S/22 | 03/3/2023 | 0+090 | RHS | 148 | 1720 | 14.2 | 1786 | 14.6 | 96 | 97 | | 777/S/22 | 03/3/2023 | 0+130 | LHS | 150 | 1776 | 14.3 | 1786 | 14.6 | 99 | 98 | |

**Eng. J. M. Mbarua**

**For: CHIEF ENGINEER (MATERIALS)**

**OiC Soils Laboratory CSE Soils Laboratory**

**………………. …………………….**